Static Call Graph - [can2usb Configuration\can2usb Configuration.axf]

# Static Call Graph for image can2usb Configuration\can2usb Configuration.axf

#<CALLGRAPH># ARM Linker, 5050169: Last Updated: Mon Sep 21 16:54:20 2015

### Maximum Stack Usage = 372 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - BusFault_Handler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - CAN1_RX0_IRQHandler from stm32f1xx_it.o(i.CAN1_RX0_IRQHandler) referenced from startup_stm32f105xc.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - CAN1_TX_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - CAN2_RX0_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - CAN2_RX1_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - CAN2_SCE_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - CAN2_TX_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - CDC_Control_FS from usbd_cdc_if.o(i.CDC_Control_FS) referenced 2 times from usbd_cdc_if.o(.data)
  - CDC_DeInit_FS from usbd_cdc_if.o(i.CDC_DeInit_FS) referenced 2 times from usbd_cdc_if.o(.data)
  - CDC_Init_FS from usbd_cdc_if.o(i.CDC_Init_FS) referenced 2 times from usbd_cdc_if.o(.data)
  - CDC_Receive_FS from usbd_cdc_if.o(i.CDC_Receive_FS) referenced 2 times from usbd_cdc_if.o(.data)
  - DMA1_Channel1_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - DMA2_Channel1_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - DMA2_Channel2_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - DMA2_Channel3_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - DMA2_Channel4_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - DMA2_Channel5_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - DebugMon_Handler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - FLASH_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - HardFault_Handler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - MemManage_Handler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - NMI_Handler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - OTG_FS_IRQHandler from stm32f1xx_it.o(i.OTG_FS_IRQHandler) referenced from startup_stm32f105xc.o(RESET)
  - OTG_FS_WKUP_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - PVD_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - PendSV_Handler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - RCC_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - RTC_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - Reset_Handler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - SPI1_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - SPI2_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - SPI3_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - SVC_Handler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - SysTick_Handler from stm32f1xx_it.o(i.SysTick_Handler) referenced from startup_stm32f105xc.o(RESET)
  - SystemInit from system_stm32f1xx.o(i.SystemInit) referenced from startup_stm32f105xc.o(.text)
  - TAMPER_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - TIM2_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - TIM3_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - TIM4_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - TIM5_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - TIM6_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - TIM7_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - UART4_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - UART5_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - USART1_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - USART2_IRQHandler from main.o(i.USART2_IRQHandler) referenced from startup_stm32f105xc.o(RESET)
  - USART3_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - USBD_CDC_DataIn from usbd_cdc.o(i.USBD_CDC_DataIn) referenced 2 times from usbd_cdc.o(.data)
  - USBD_CDC_DataOut from usbd_cdc.o(i.USBD_CDC_DataOut) referenced 2 times from usbd_cdc.o(.data)
  - USBD_CDC_DeInit from usbd_cdc.o(i.USBD_CDC_DeInit) referenced 2 times from usbd_cdc.o(.data)
  - USBD_CDC_EP0_RxReady from usbd_cdc.o(i.USBD_CDC_EP0_RxReady) referenced 2 times from usbd_cdc.o(.data)
  - USBD_CDC_GetDeviceQualifierDescriptor from usbd_cdc.o(i.USBD_CDC_GetDeviceQualifierDescriptor) referenced 2 times from usbd_cdc.o(.data)
  - USBD_CDC_GetFSCfgDesc from usbd_cdc.o(i.USBD_CDC_GetFSCfgDesc) referenced 2 times from usbd_cdc.o(.data)
  - USBD_CDC_GetHSCfgDesc from usbd_cdc.o(i.USBD_CDC_GetHSCfgDesc) referenced 2 times from usbd_cdc.o(.data)
  - USBD_CDC_GetOtherSpeedCfgDesc from usbd_cdc.o(i.USBD_CDC_GetOtherSpeedCfgDesc) referenced 2 times from usbd_cdc.o(.data)
  - USBD_CDC_Init from usbd_cdc.o(i.USBD_CDC_Init) referenced 2 times from usbd_cdc.o(.data)
  - USBD_CDC_Setup from usbd_cdc.o(i.USBD_CDC_Setup) referenced 2 times from usbd_cdc.o(.data)
  - USBD_FS_ConfigStrDescriptor from usbd_desc.o(i.USBD_FS_ConfigStrDescriptor) referenced 2 times from usbd_desc.o(.data)
  - USBD_FS_DeviceDescriptor from usbd_desc.o(i.USBD_FS_DeviceDescriptor) referenced 2 times from usbd_desc.o(.data)
  - USBD_FS_InterfaceStrDescriptor from usbd_desc.o(i.USBD_FS_InterfaceStrDescriptor) referenced 2 times from usbd_desc.o(.data)
  - USBD_FS_LangIDStrDescriptor from usbd_desc.o(i.USBD_FS_LangIDStrDescriptor) referenced 2 times from usbd_desc.o(.data)
  - USBD_FS_ManufacturerStrDescriptor from usbd_desc.o(i.USBD_FS_ManufacturerStrDescriptor) referenced 2 times from usbd_desc.o(.data)
  - USBD_FS_ProductStrDescriptor from usbd_desc.o(i.USBD_FS_ProductStrDescriptor) referenced 2 times from usbd_desc.o(.data)
  - USBD_FS_SerialStrDescriptor from usbd_desc.o(i.USBD_FS_SerialStrDescriptor) referenced 2 times from usbd_desc.o(.data)
  - UsageFault_Handler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - WWDG_IRQHandler from startup_stm32f105xc.o(.text) referenced from startup_stm32f105xc.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f105xc.o(.text)
  - _sputc from printf8.o(i._sputc) referenced from printf8.o(i.__0sprintf$8)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_stm32f105xc.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f105xc.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f105xc.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f105xc.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f105xc.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_stm32f105xc.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_stm32f105xc.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_stm32f105xc.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f105xc.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  CAN2_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  CAN2_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  CAN2_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  CAN2_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  DMA2_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  DMA2_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f105xc.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_uldivmod

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  __aeabi_memcpy (Thumb, 36 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> HAL_PCD_Init

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _printf_core

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_uldivmod

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __decompress (Thumb, 0 bytes, Stack size unknown bytes, __dczerorl2.o(.text), UNUSED)

  __decompress1 (Thumb, 86 bytes, Stack size unknown bytes, __dczerorl2.o(.text), UNUSED)

  CAN1_RX0_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.CAN1_RX0_IRQHandler))
  [Stack]

  - Max Depth = 248
  - Call Chain = CAN1_RX0_IRQHandler ⇒ HAL_CAN_IRQHandler ⇒ CAN_Receive_IT ⇒ HAL_CAN_RxCpltCallback ⇒ led_blink
  [Calls]
  - >> HAL_CAN_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f105xc.o(RESET)

  CDC_Transmit_FS (Thumb, 24 bytes, Stack size 8 bytes, usbd_cdc_if.o(i.CDC_Transmit_FS))
  [Stack]

  - Max Depth = 60
  - Call Chain = CDC_Transmit_FS ⇒ USBD_CDC_TransmitPacket ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_CDC_TransmitPacket
  - >> USBD_CDC_SetTxBuffer
  [Called By]
  - >> usb_access

  CDC_add_buf_to_transmit (Thumb, 44 bytes, Stack size 16 bytes, usbd_cdc_if.o(i.CDC_add_buf_to_transmit))
  [Stack]

  - Max Depth = 16
  - Call Chain = CDC_add_buf_to_transmit
  [Called By]
  - >> HAL_CAN_RxCpltCallback

  CDC_periodic_callback (Thumb, 80 bytes, Stack size 16 bytes, usbd_cdc_if.o(i.CDC_periodic_callback))
  [Stack]

  - Max Depth = 68
  - Call Chain = CDC_periodic_callback ⇒ USBD_CDC_TransmitPacket ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_CDC_TransmitPacket
  - >> USBD_CDC_SetTxBuffer
  [Called By]
  - >> main

  Delay_ms (Thumb, 18 bytes, Stack size 0 bytes, main.o(i.Delay_ms))
  [Called By]

  - >> main
  - >> led_blink

  HAL_CAN_ConfigFilter (Thumb, 242 bytes, Stack size 20 bytes, stm32f1xx_hal_can.o(i.HAL_CAN_ConfigFilter))
  [Stack]

  - Max Depth = 20
  - Call Chain = HAL_CAN_ConfigFilter
  [Called By]
  - >> main

  HAL_CAN_ErrorCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_can.o(i.HAL_CAN_ErrorCallback))
  [Called By]

  - >> HAL_CAN_IRQHandler

  HAL_CAN_IRQHandler (Thumb, 378 bytes, Stack size 16 bytes, stm32f1xx_hal_can.o(i.HAL_CAN_IRQHandler))
  [Stack]

  - Max Depth = 248
  - Call Chain = HAL_CAN_IRQHandler ⇒ CAN_Receive_IT ⇒ HAL_CAN_RxCpltCallback ⇒ led_blink
  [Calls]
  - >> HAL_CAN_TxCpltCallback
  - >> HAL_CAN_ErrorCallback
  - >> CAN_Receive_IT
  [Called By]
  - >> CAN1_RX0_IRQHandler

  HAL_CAN_Init (Thumb, 274 bytes, Stack size 24 bytes, stm32f1xx_hal_can.o(i.HAL_CAN_Init))
  [Stack]

  - Max Depth = 96
  - Call Chain = HAL_CAN_Init ⇒ HAL_CAN_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_CAN_MspInit
  - >> HAL_GetTick
  [Called By]
  - >> MX_CAN1_Init

  HAL_CAN_MspInit (Thumb, 106 bytes, Stack size 32 bytes, stm32f1xx_hal_msp.o(i.HAL_CAN_MspInit))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_CAN_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_GPIO_Init
  [Called By]
  - >> HAL_CAN_Init

  HAL_CAN_Receive_IT (Thumb, 100 bytes, Stack size 12 bytes, stm32f1xx_hal_can.o(i.HAL_CAN_Receive_IT))
  [Stack]

  - Max Depth = 12
  - Call Chain = HAL_CAN_Receive_IT
  [Called By]
  - >> main
  - >> HAL_CAN_RxCpltCallback

  HAL_CAN_RxCpltCallback (Thumb, 408 bytes, Stack size 208 bytes, main.o(i.HAL_CAN_RxCpltCallback))
  [Stack]

  - Max Depth = 224
  - Call Chain = HAL_CAN_RxCpltCallback ⇒ led_blink
  [Calls]
  - >> HAL_CAN_Receive_IT
  - >> led_blink
  - >> halfbyte_to_hexascii
  - >> CDC_add_buf_to_transmit
  [Called By]
  - >> CAN_Receive_IT

  HAL_CAN_Transmit (Thumb, 412 bytes, Stack size 40 bytes, stm32f1xx_hal_can.o(i.HAL_CAN_Transmit))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_CAN_Transmit
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> main
  - >> CDC_Receive_FS

  HAL_CAN_TxCpltCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_can.o(i.HAL_CAN_TxCpltCallback))
  [Called By]

  - >> HAL_CAN_IRQHandler

  HAL_Delay (Thumb, 22 bytes, Stack size 16 bytes, stm32f1xx_hal.o(i.HAL_Delay))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_Delay
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> HAL_RCC_OscConfig
  - >> USB_SetCurrentMode
  - >> USB_DevDisconnect
  - >> USB_DevConnect

  HAL_GPIO_Init (Thumb, 408 bytes, Stack size 40 bytes, stm32f1xx_hal_gpio.o(i.HAL_GPIO_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_GPIO_Init
  [Called By]
  - >> HAL_PCD_MspInit
  - >> HAL_UART_MspInit
  - >> HAL_CAN_MspInit
  - >> MX_GPIO_Init

  HAL_GetTick (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_hal.o(i.HAL_GetTick))
  [Called By]

  - >> HAL_Delay
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  - >> HAL_RCCEx_PeriphCLKConfig
  - >> HAL_CAN_Init
  - >> HAL_CAN_Transmit

  HAL_IncTick (Thumb, 10 bytes, Stack size 0 bytes, stm32f1xx_hal.o(i.HAL_IncTick))
  [Called By]

  - >> SysTick_Handler

  HAL_Init (Thumb, 32 bytes, Stack size 8 bytes, stm32f1xx_hal.o(i.HAL_Init))
  [Stack]

  - Max Depth = 84
  - Call Chain = HAL_Init ⇒ HAL_InitTick ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_NVIC_SetPriorityGrouping
  - >> HAL_MspInit
  - >> HAL_InitTick
  [Called By]
  - >> main

  HAL_InitTick (Thumb, 34 bytes, Stack size 8 bytes, stm32f1xx_hal.o(i.HAL_InitTick))
  [Stack]

  - Max Depth = 76
  - Call Chain = HAL_InitTick ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_SYSTICK_Config
  - >> HAL_RCC_GetHCLKFreq
  [Called By]
  - >> HAL_RCC_ClockConfig
  - >> HAL_Init

  HAL_MspInit (Thumb, 52 bytes, Stack size 8 bytes, stm32f1xx_hal_msp.o(i.HAL_MspInit))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_MspInit ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriorityGrouping
  - >> HAL_NVIC_SetPriority
  [Called By]
  - >> HAL_Init

  HAL_NVIC_EnableIRQ (Thumb, 22 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.HAL_NVIC_EnableIRQ))
  [Called By]

  - >> HAL_PCD_MspInit
  - >> HAL_CAN_MspInit

  HAL_NVIC_SetPriority (Thumb, 60 bytes, Stack size 16 bytes, stm32f1xx_hal_cortex.o(i.HAL_NVIC_SetPriority))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_NVIC_SetPriority
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> HAL_PCD_MspInit
  - >> HAL_MspInit
  - >> HAL_CAN_MspInit
  - >> HAL_InitTick

  HAL_NVIC_SetPriorityGrouping (Thumb, 26 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.HAL_NVIC_SetPriorityGrouping))
  [Called By]

  - >> HAL_MspInit
  - >> HAL_Init

  HAL_PCDEx_SetConnectionState (Thumb, 2 bytes, Stack size 0 bytes, usbd_conf.o(i.HAL_PCDEx_SetConnectionState))
  [Called By]

  - >> HAL_PCD_Start

  HAL_PCDEx_SetRxFiFo (Thumb, 8 bytes, Stack size 0 bytes, stm32f1xx_hal_pcd_ex.o(i.HAL_PCDEx_SetRxFiFo))
  [Called By]

  - >> USBD_LL_Init

  HAL_PCDEx_SetTxFiFo (Thumb, 68 bytes, Stack size 20 bytes, stm32f1xx_hal_pcd_ex.o(i.HAL_PCDEx_SetTxFiFo))
  [Stack]

  - Max Depth = 20
  - Call Chain = HAL_PCDEx_SetTxFiFo
  [Called By]
  - >> USBD_LL_Init

  HAL_PCD_ConnectCallback (Thumb, 8 bytes, Stack size 0 bytes, usbd_conf.o(i.HAL_PCD_ConnectCallback))
  [Calls]

  - >> USBD_LL_DevConnected
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_PCD_DataInStageCallback (Thumb, 18 bytes, Stack size 0 bytes, usbd_conf.o(i.HAL_PCD_DataInStageCallback))
  [Stack]

  - Max Depth = 76
  - Call Chain = HAL_PCD_DataInStageCallback ⇒ USBD_LL_DataInStage ⇒ USBD_CtlReceiveStatus ⇒ USBD_LL_PrepareReceive ⇒ HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_DataInStage
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_PCD_DataOutStageCallback (Thumb, 20 bytes, Stack size 0 bytes, usbd_conf.o(i.HAL_PCD_DataOutStageCallback))
  [Stack]

  - Max Depth = 68
  - Call Chain = HAL_PCD_DataOutStageCallback ⇒ USBD_LL_DataOutStage ⇒ USBD_CtlSendStatus ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_DataOutStage
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_PCD_DisconnectCallback (Thumb, 8 bytes, Stack size 0 bytes, usbd_conf.o(i.HAL_PCD_DisconnectCallback))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_PCD_DisconnectCallback ⇒ USBD_LL_DevDisconnected
  [Calls]
  - >> USBD_LL_DevDisconnected
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_PCD_EP_Close (Thumb, 68 bytes, Stack size 8 bytes, stm32f1xx_hal_pcd.o(i.HAL_PCD_EP_Close))
  [Stack]

  - Max Depth = 20
  - Call Chain = HAL_PCD_EP_Close ⇒ USB_DeactivateEndpoint
  [Calls]
  - >> USB_DeactivateEndpoint
  [Called By]
  - >> USBD_LL_CloseEP

  HAL_PCD_EP_ClrStall (Thumb, 80 bytes, Stack size 16 bytes, stm32f1xx_hal_pcd.o(i.HAL_PCD_EP_ClrStall))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_PCD_EP_ClrStall
  [Calls]
  - >> USB_EPClearStall
  [Called By]
  - >> USBD_LL_ClearStallEP

  HAL_PCD_EP_GetRxCount (Thumb, 20 bytes, Stack size 0 bytes, stm32f1xx_hal_pcd.o(i.HAL_PCD_EP_GetRxCount))
  [Called By]

  - >> USBD_LL_GetRxDataSize

  HAL_PCD_EP_Open (Thumb, 72 bytes, Stack size 16 bytes, stm32f1xx_hal_pcd.o(i.HAL_PCD_EP_Open))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_PCD_EP_Open ⇒ USB_ActivateEndpoint
  [Calls]
  - >> USB_ActivateEndpoint
  [Called By]
  - >> USBD_LL_OpenEP

  HAL_PCD_EP_Receive (Thumb, 82 bytes, Stack size 16 bytes, stm32f1xx_hal_pcd.o(i.HAL_PCD_EP_Receive))
  [Stack]

  - Max Depth = 36
  - Call Chain = HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USB_EPStartXfer
  - >> USB_EP0StartXfer
  [Called By]
  - >> USBD_LL_PrepareReceive

  HAL_PCD_EP_SetStall (Thumb, 94 bytes, Stack size 16 bytes, stm32f1xx_hal_pcd.o(i.HAL_PCD_EP_SetStall))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_PCD_EP_SetStall
  [Calls]
  - >> USB_EPSetStall
  - >> USB_EP0_OutStart
  [Called By]
  - >> USBD_LL_StallEP

  HAL_PCD_EP_Transmit (Thumb, 78 bytes, Stack size 16 bytes, stm32f1xx_hal_pcd.o(i.HAL_PCD_EP_Transmit))
  [Stack]

  - Max Depth = 36
  - Call Chain = HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USB_EPStartXfer
  - >> USB_EP0StartXfer
  [Called By]
  - >> USBD_LL_Transmit

  HAL_PCD_IRQHandler (Thumb, 826 bytes, Stack size 40 bytes, stm32f1xx_hal_pcd.o(i.HAL_PCD_IRQHandler))
  [Stack]

  - Max Depth = 156
  - Call Chain = HAL_PCD_IRQHandler ⇒ HAL_PCD_SetupStageCallback ⇒ USBD_LL_SetupStage ⇒ USBD_StdDevReq ⇒ USBD_GetDescriptor ⇒ USBD_CtlSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> HAL_PCD_SuspendCallback
  - >> HAL_PCD_SetupStageCallback
  - >> HAL_PCD_SOFCallback
  - >> HAL_PCD_ResumeCallback
  - >> HAL_PCD_ResetCallback
  - >> HAL_PCD_ISOOUTIncompleteCallback
  - >> HAL_PCD_ISOINIncompleteCallback
  - >> HAL_PCD_DisconnectCallback
  - >> HAL_PCD_DataOutStageCallback
  - >> HAL_PCD_DataInStageCallback
  - >> HAL_PCD_ConnectCallback
  - >> USB_ReadPacket
  - >> USB_ReadInterrupts
  - >> USB_ReadDevOutEPInterrupt
  - >> USB_ReadDevInEPInterrupt
  - >> USB_ReadDevAllOutEpInterrupt
  - >> USB_ReadDevAllInEpInterrupt
  - >> USB_GetMode
  - >> USB_FlushTxFifo
  - >> USB_EP0_OutStart
  - >> USB_ActivateSetup
  - >> PCD_WriteEmptyTxFifo
  [Called By]
  - >> OTG_FS_IRQHandler

  HAL_PCD_ISOINIncompleteCallback (Thumb, 8 bytes, Stack size 0 bytes, usbd_conf.o(i.HAL_PCD_ISOINIncompleteCallback))
  [Calls]

  - >> USBD_LL_IsoINIncomplete
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_PCD_ISOOUTIncompleteCallback (Thumb, 8 bytes, Stack size 0 bytes, usbd_conf.o(i.HAL_PCD_ISOOUTIncompleteCallback))
  [Calls]

  - >> USBD_LL_IsoOUTIncomplete
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_PCD_Init (Thumb, 200 bytes, Stack size 48 bytes, stm32f1xx_hal_pcd.o(i.HAL_PCD_Init))
  [Stack]

  - Max Depth = 112
  - Call Chain = HAL_PCD_Init ⇒ HAL_PCD_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_PCD_MspInit
  - >> USB_SetCurrentMode
  - >> USB_DisableGlobalInt
  - >> USB_DevInit
  - >> USB_DevDisconnect
  - >> USB_CoreInit
  - >> __aeabi_memcpy4
  [Called By]
  - >> USBD_LL_Init

  HAL_PCD_MspInit (Thumb, 70 bytes, Stack size 24 bytes, usbd_conf.o(i.HAL_PCD_MspInit))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_PCD_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_GPIO_Init
  [Called By]
  - >> HAL_PCD_Init

  HAL_PCD_ResetCallback (Thumb, 32 bytes, Stack size 8 bytes, usbd_conf.o(i.HAL_PCD_ResetCallback))
  [Stack]

  - Max Depth = 60
  - Call Chain = HAL_PCD_ResetCallback ⇒ USBD_LL_Reset ⇒ USBD_LL_OpenEP ⇒ HAL_PCD_EP_Open ⇒ USB_ActivateEndpoint
  [Calls]
  - >> USBD_LL_SetSpeed
  - >> USBD_LL_Reset
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_PCD_ResumeCallback (Thumb, 8 bytes, Stack size 0 bytes, usbd_conf.o(i.HAL_PCD_ResumeCallback))
  [Calls]

  - >> USBD_LL_Resume
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_PCD_SOFCallback (Thumb, 8 bytes, Stack size 0 bytes, usbd_conf.o(i.HAL_PCD_SOFCallback))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_PCD_SOFCallback ⇒ USBD_LL_SOF
  [Calls]
  - >> USBD_LL_SOF
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_PCD_SetAddress (Thumb, 40 bytes, Stack size 8 bytes, stm32f1xx_hal_pcd.o(i.HAL_PCD_SetAddress))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_PCD_SetAddress
  [Calls]
  - >> USB_SetDevAddress
  [Called By]
  - >> USBD_LL_SetUSBAddress

  HAL_PCD_SetupStageCallback (Thumb, 14 bytes, Stack size 0 bytes, usbd_conf.o(i.HAL_PCD_SetupStageCallback))
  [Stack]

  - Max Depth = 116
  - Call Chain = HAL_PCD_SetupStageCallback ⇒ USBD_LL_SetupStage ⇒ USBD_StdDevReq ⇒ USBD_GetDescriptor ⇒ USBD_CtlSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_SetupStage
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_PCD_Start (Thumb, 50 bytes, Stack size 8 bytes, stm32f1xx_hal_pcd.o(i.HAL_PCD_Start))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_PCD_Start ⇒ USB_DevConnect ⇒ HAL_Delay
  [Calls]
  - >> HAL_PCDEx_SetConnectionState
  - >> USB_EnableGlobalInt
  - >> USB_DevConnect
  [Called By]
  - >> USBD_LL_Start

  HAL_PCD_SuspendCallback (Thumb, 44 bytes, Stack size 8 bytes, usbd_conf.o(i.HAL_PCD_SuspendCallback))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_PCD_SuspendCallback
  [Calls]
  - >> USBD_LL_Suspend
  [Called By]
  - >> HAL_PCD_IRQHandler

  HAL_RCCEx_PeriphCLKConfig (Thumb, 502 bytes, Stack size 40 bytes, stm32f1xx_hal_rcc_ex.o(i.HAL_RCCEx_PeriphCLKConfig))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_RCCEx_PeriphCLKConfig
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_ClockConfig (Thumb, 638 bytes, Stack size 32 bytes, stm32f1xx_hal_rcc_ex.o(i.HAL_RCC_ClockConfig))
  [Stack]

  - Max Depth = 108
  - Call Chain = HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_InitTick
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_GetHCLKFreq (Thumb, 38 bytes, Stack size 8 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetHCLKFreq))
  [Stack]

  - Max Depth = 68
  - Call Chain = HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_GetSysClockFreq
  [Called By]
  - >> SystemClock_Config
  - >> HAL_RCC_GetPCLK2Freq
  - >> HAL_InitTick
  - >> HAL_RCC_GetPCLK1Freq

  HAL_RCC_GetPCLK1Freq (Thumb, 36 bytes, Stack size 8 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq))
  [Stack]

  - Max Depth = 76
  - Call Chain = HAL_RCC_GetPCLK1Freq ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_GetHCLKFreq
  [Called By]
  - >> UART_SetConfig

  HAL_RCC_GetPCLK2Freq (Thumb, 36 bytes, Stack size 8 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq))
  [Stack]

  - Max Depth = 76
  - Call Chain = HAL_RCC_GetPCLK2Freq ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_GetHCLKFreq
  [Called By]
  - >> UART_SetConfig

  HAL_RCC_GetSysClockFreq (Thumb, 180 bytes, Stack size 60 bytes, stm32f1xx_hal_rcc_ex.o(i.HAL_RCC_GetSysClockFreq))
  [Stack]

  - Max Depth = 60
  - Call Chain = HAL_RCC_GetSysClockFreq
  [Called By]
  - >> HAL_RCC_GetHCLKFreq

  HAL_RCC_OscConfig (Thumb, 2038 bytes, Stack size 40 bytes, stm32f1xx_hal_rcc_ex.o(i.HAL_RCC_OscConfig))
  [Stack]

  - Max Depth = 56
  - Call Chain = HAL_RCC_OscConfig ⇒ HAL_Delay
  [Calls]
  - >> HAL_Delay
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_SYSTICK_CLKSourceConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_CLKSourceConfig))
  [Called By]

  - >> SystemClock_Config

  HAL_SYSTICK_Callback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_Callback))
  [Called By]

  - >> HAL_SYSTICK_IRQHandler

  HAL_SYSTICK_Config (Thumb, 40 bytes, Stack size 8 bytes, stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_Config))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SYSTICK_Config
  [Calls]
  - >> NVIC_SetPriority
  [Called By]
  - >> SystemClock_Config
  - >> HAL_InitTick

  HAL_SYSTICK_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SYSTICK_IRQHandler
  [Calls]
  - >> HAL_SYSTICK_Callback
  [Called By]
  - >> SysTick_Handler

  HAL_TIMEx_MasterConfigSynchronization (Thumb, 80 bytes, Stack size 12 bytes, stm32f1xx_hal_tim_ex.o(i.HAL_TIMEx_MasterConfigSynchronization))
  [Stack]

  - Max Depth = 12
  - Call Chain = HAL_TIMEx_MasterConfigSynchronization
  [Called By]
  - >> MX_TIM1_Init

  HAL_TIM_Base_Init (Thumb, 54 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_Base_Init))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_TIM_Base_Init ⇒ TIM_Base_SetConfig
  [Calls]
  - >> HAL_TIM_Base_MspInit
  - >> TIM_Base_SetConfig
  [Called By]
  - >> MX_TIM1_Init

  HAL_TIM_Base_MspInit (Thumb, 30 bytes, Stack size 8 bytes, stm32f1xx_hal_msp.o(i.HAL_TIM_Base_MspInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_TIM_Base_MspInit
  [Called By]
  - >> HAL_TIM_Base_Init

  HAL_TIM_Base_Start (Thumb, 26 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_Base_Start))
  [Called By]

  - >> main

  HAL_TIM_ConfigClockSource (Thumb, 242 bytes, Stack size 16 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_ConfigClockSource))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_TIM_ConfigClockSource ⇒ TIM_TI2_ConfigInputStage
  [Calls]
  - >> TIM_TI2_ConfigInputStage
  - >> TIM_TI1_ConfigInputStage
  - >> TIM_ITRx_SetConfig
  - >> TIM_ETR_SetConfig
  [Called By]
  - >> MX_TIM1_Init

  HAL_UART_Init (Thumb, 94 bytes, Stack size 16 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_Init))
  [Stack]

  - Max Depth = 116
  - Call Chain = HAL_UART_Init ⇒ UART_SetConfig ⇒ HAL_RCC_GetPCLK2Freq ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_UART_MspInit
  - >> UART_SetConfig
  [Called By]
  - >> main

  HAL_UART_MspInit (Thumb, 74 bytes, Stack size 32 bytes, stm32f1xx_hal_msp.o(i.HAL_UART_MspInit))
  [Stack]

  - Max Depth = 72
  - Call Chain = HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> HAL_UART_Init

  MX_USB_DEVICE_Init (Thumb, 38 bytes, Stack size 8 bytes, usb_device.o(i.MX_USB_DEVICE_Init))
  [Stack]

  - Max Depth = 136
  - Call Chain = MX_USB_DEVICE_Init ⇒ USBD_Init ⇒ USBD_LL_Init ⇒ HAL_PCD_Init ⇒ HAL_PCD_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> USBD_Start
  - >> USBD_RegisterClass
  - >> USBD_Init
  - >> USBD_CDC_RegisterInterface
  [Called By]
  - >> main

  OTG_FS_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.OTG_FS_IRQHandler))
  [Stack]

  - Max Depth = 156
  - Call Chain = OTG_FS_IRQHandler ⇒ HAL_PCD_IRQHandler ⇒ HAL_PCD_SetupStageCallback ⇒ USBD_LL_SetupStage ⇒ USBD_StdDevReq ⇒ USBD_GetDescriptor ⇒ USBD_CtlSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> HAL_PCD_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f105xc.o(RESET)

  SysTick_Handler (Thumb, 14 bytes, Stack size 8 bytes, stm32f1xx_it.o(i.SysTick_Handler))
  [Stack]

  - Max Depth = 16
  - Call Chain = SysTick_Handler ⇒ HAL_SYSTICK_IRQHandler
  [Calls]
  - >> HAL_SYSTICK_IRQHandler
  - >> HAL_IncTick
  [Address Reference Count : 1]
  - startup_stm32f105xc.o(RESET)

  SystemClock_Config (Thumb, 118 bytes, Stack size 128 bytes, main.o(i.SystemClock_Config))
  [Stack]

  - Max Depth = 236
  - Call Chain = SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_SYSTICK_Config
  - >> HAL_SYSTICK_CLKSourceConfig
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_GetHCLKFreq
  - >> HAL_RCC_ClockConfig
  - >> HAL_RCCEx_PeriphCLKConfig
  [Called By]
  - >> main

  SystemInit (Thumb, 68 bytes, Stack size 0 bytes, system_stm32f1xx.o(i.SystemInit))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(.text)

  TIM_Base_SetConfig (Thumb, 98 bytes, Stack size 20 bytes, stm32f1xx_hal_tim.o(i.TIM_Base_SetConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = TIM_Base_SetConfig
  [Called By]
  - >> HAL_TIM_Base_Init

  USART2_IRQHandler (Thumb, 38 bytes, Stack size 0 bytes, main.o(i.USART2_IRQHandler))
  [Address Reference Count : 1]

  - startup_stm32f105xc.o(RESET)

  USBD_CDC_GetDeviceQualifierDescriptor (Thumb, 8 bytes, Stack size 0 bytes, usbd_cdc.o(i.USBD_CDC_GetDeviceQualifierDescriptor))
  [Address Reference Count : 1]

  - usbd_cdc.o(.data)

  USBD_CDC_ReceivePacket (Thumb, 40 bytes, Stack size 8 bytes, usbd_cdc.o(i.USBD_CDC_ReceivePacket))
  [Stack]

  - Max Depth = 52
  - Call Chain = USBD_CDC_ReceivePacket ⇒ USBD_LL_PrepareReceive ⇒ HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_PrepareReceive
  [Called By]
  - >> CDC_Receive_FS

  USBD_CDC_RegisterInterface (Thumb, 16 bytes, Stack size 0 bytes, usbd_cdc.o(i.USBD_CDC_RegisterInterface))
  [Called By]

  - >> MX_USB_DEVICE_Init

  USBD_CDC_SetRxBuffer (Thumb, 12 bytes, Stack size 0 bytes, usbd_cdc.o(i.USBD_CDC_SetRxBuffer))
  [Called By]

  - >> CDC_Receive_FS
  - >> CDC_Init_FS

  USBD_CDC_SetTxBuffer (Thumb, 16 bytes, Stack size 0 bytes, usbd_cdc.o(i.USBD_CDC_SetTxBuffer))
  [Called By]

  - >> CDC_periodic_callback
  - >> CDC_Transmit_FS
  - >> CDC_Init_FS

  USBD_CDC_TransmitPacket (Thumb, 48 bytes, Stack size 8 bytes, usbd_cdc.o(i.USBD_CDC_TransmitPacket))
  [Stack]

  - Max Depth = 52
  - Call Chain = USBD_CDC_TransmitPacket ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_Transmit
  [Called By]
  - >> CDC_periodic_callback
  - >> CDC_Transmit_FS

  USBD_ClrClassConfig (Thumb, 14 bytes, Stack size 8 bytes, usbd_core.o(i.USBD_ClrClassConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = USBD_ClrClassConfig
  [Called By]
  - >> USBD_SetConfig

  USBD_CtlContinueRx (Thumb, 16 bytes, Stack size 8 bytes, usbd_ioreq.o(i.USBD_CtlContinueRx))
  [Stack]

  - Max Depth = 52
  - Call Chain = USBD_CtlContinueRx ⇒ USBD_LL_PrepareReceive ⇒ HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_PrepareReceive
  [Called By]
  - >> USBD_LL_DataOutStage

  USBD_CtlContinueSendData (Thumb, 16 bytes, Stack size 8 bytes, usbd_ioreq.o(i.USBD_CtlContinueSendData))
  [Stack]

  - Max Depth = 52
  - Call Chain = USBD_CtlContinueSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_Transmit
  [Called By]
  - >> USBD_LL_DataInStage

  USBD_CtlError (Thumb, 22 bytes, Stack size 8 bytes, usbd_ctlreq.o(i.USBD_CtlError))
  [Stack]

  - Max Depth = 32
  - Call Chain = USBD_CtlError ⇒ USBD_LL_StallEP ⇒ HAL_PCD_EP_SetStall
  [Calls]
  - >> USBD_LL_StallEP
  [Called By]
  - >> USBD_SetConfig
  - >> USBD_GetDescriptor
  - >> USBD_StdItfReq
  - >> USBD_StdEPReq
  - >> USBD_StdDevReq

  USBD_CtlPrepareRx (Thumb, 30 bytes, Stack size 8 bytes, usbd_ioreq.o(i.USBD_CtlPrepareRx))
  [Stack]

  - Max Depth = 52
  - Call Chain = USBD_CtlPrepareRx ⇒ USBD_LL_PrepareReceive ⇒ HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_PrepareReceive
  [Called By]
  - >> USBD_CDC_Setup

  USBD_CtlReceiveStatus (Thumb, 22 bytes, Stack size 8 bytes, usbd_ioreq.o(i.USBD_CtlReceiveStatus))
  [Stack]

  - Max Depth = 52
  - Call Chain = USBD_CtlReceiveStatus ⇒ USBD_LL_PrepareReceive ⇒ HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_PrepareReceive
  [Called By]
  - >> USBD_LL_DataInStage

  USBD_CtlSendData (Thumb, 26 bytes, Stack size 8 bytes, usbd_ioreq.o(i.USBD_CtlSendData))
  [Stack]

  - Max Depth = 52
  - Call Chain = USBD_CtlSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_Transmit
  [Called By]
  - >> USBD_GetDescriptor
  - >> USBD_StdEPReq
  - >> USBD_StdDevReq
  - >> USBD_CDC_Setup

  USBD_CtlSendStatus (Thumb, 22 bytes, Stack size 8 bytes, usbd_ioreq.o(i.USBD_CtlSendStatus))
  [Stack]

  - Max Depth = 52
  - Call Chain = USBD_CtlSendStatus ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_Transmit
  [Called By]
  - >> USBD_LL_DataOutStage
  - >> USBD_SetConfig
  - >> USBD_StdItfReq
  - >> USBD_StdEPReq
  - >> USBD_StdDevReq

  USBD_FS_ConfigStrDescriptor (Thumb, 16 bytes, Stack size 8 bytes, usbd_desc.o(i.USBD_FS_ConfigStrDescriptor))
  [Stack]

  - Max Depth = 24
  - Call Chain = USBD_FS_ConfigStrDescriptor ⇒ USBD_GetString
  [Calls]
  - >> USBD_GetString
  [Address Reference Count : 1]
  - usbd_desc.o(.data)

  USBD_FS_DeviceDescriptor (Thumb, 8 bytes, Stack size 0 bytes, usbd_desc.o(i.USBD_FS_DeviceDescriptor))
  [Address Reference Count : 1]

  - usbd_desc.o(.data)

  USBD_FS_InterfaceStrDescriptor (Thumb, 16 bytes, Stack size 8 bytes, usbd_desc.o(i.USBD_FS_InterfaceStrDescriptor))
  [Stack]

  - Max Depth = 24
  - Call Chain = USBD_FS_InterfaceStrDescriptor ⇒ USBD_GetString
  [Calls]
  - >> USBD_GetString
  [Address Reference Count : 1]
  - usbd_desc.o(.data)

  USBD_FS_LangIDStrDescriptor (Thumb, 8 bytes, Stack size 0 bytes, usbd_desc.o(i.USBD_FS_LangIDStrDescriptor))
  [Address Reference Count : 1]

  - usbd_desc.o(.data)

  USBD_FS_ManufacturerStrDescriptor (Thumb, 16 bytes, Stack size 8 bytes, usbd_desc.o(i.USBD_FS_ManufacturerStrDescriptor))
  [Stack]

  - Max Depth = 24
  - Call Chain = USBD_FS_ManufacturerStrDescriptor ⇒ USBD_GetString
  [Calls]
  - >> USBD_GetString
  [Address Reference Count : 1]
  - usbd_desc.o(.data)

  USBD_FS_ProductStrDescriptor (Thumb, 16 bytes, Stack size 8 bytes, usbd_desc.o(i.USBD_FS_ProductStrDescriptor))
  [Stack]

  - Max Depth = 24
  - Call Chain = USBD_FS_ProductStrDescriptor ⇒ USBD_GetString
  [Calls]
  - >> USBD_GetString
  [Address Reference Count : 1]
  - usbd_desc.o(.data)

  USBD_FS_SerialStrDescriptor (Thumb, 16 bytes, Stack size 8 bytes, usbd_desc.o(i.USBD_FS_SerialStrDescriptor))
  [Stack]

  - Max Depth = 24
  - Call Chain = USBD_FS_SerialStrDescriptor ⇒ USBD_GetString
  [Calls]
  - >> USBD_GetString
  [Address Reference Count : 1]
  - usbd_desc.o(.data)

  USBD_GetString (Thumb, 70 bytes, Stack size 16 bytes, usbd_ctlreq.o(i.USBD_GetString))
  [Stack]

  - Max Depth = 16
  - Call Chain = USBD_GetString
  [Called By]
  - >> USBD_FS_SerialStrDescriptor
  - >> USBD_FS_ProductStrDescriptor
  - >> USBD_FS_ManufacturerStrDescriptor
  - >> USBD_FS_InterfaceStrDescriptor
  - >> USBD_FS_ConfigStrDescriptor

  USBD_Init (Thumb, 42 bytes, Stack size 8 bytes, usbd_core.o(i.USBD_Init))
  [Stack]

  - Max Depth = 128
  - Call Chain = USBD_Init ⇒ USBD_LL_Init ⇒ HAL_PCD_Init ⇒ HAL_PCD_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> USBD_LL_Init
  [Called By]
  - >> MX_USB_DEVICE_Init

  USBD_LL_ClearStallEP (Thumb, 14 bytes, Stack size 8 bytes, usbd_conf.o(i.USBD_LL_ClearStallEP))
  [Stack]

  - Max Depth = 24
  - Call Chain = USBD_LL_ClearStallEP ⇒ HAL_PCD_EP_ClrStall
  [Calls]
  - >> HAL_PCD_EP_ClrStall
  [Called By]
  - >> USBD_StdEPReq

  USBD_LL_CloseEP (Thumb, 14 bytes, Stack size 8 bytes, usbd_conf.o(i.USBD_LL_CloseEP))
  [Stack]

  - Max Depth = 28
  - Call Chain = USBD_LL_CloseEP ⇒ HAL_PCD_EP_Close ⇒ USB_DeactivateEndpoint
  [Calls]
  - >> HAL_PCD_EP_Close
  [Called By]
  - >> USBD_CDC_DeInit

  USBD_LL_DataInStage (Thumb, 160 bytes, Stack size 24 bytes, usbd_core.o(i.USBD_LL_DataInStage))
  [Stack]

  - Max Depth = 76
  - Call Chain = USBD_LL_DataInStage ⇒ USBD_CtlReceiveStatus ⇒ USBD_LL_PrepareReceive ⇒ HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_CtlReceiveStatus
  - >> USBD_CtlContinueSendData
  [Called By]
  - >> HAL_PCD_DataInStageCallback

  USBD_LL_DataOutStage (Thumb, 106 bytes, Stack size 16 bytes, usbd_core.o(i.USBD_LL_DataOutStage))
  [Stack]

  - Max Depth = 68
  - Call Chain = USBD_LL_DataOutStage ⇒ USBD_CtlSendStatus ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_CtlSendStatus
  - >> USBD_CtlContinueRx
  [Called By]
  - >> HAL_PCD_DataOutStageCallback

  USBD_LL_DevConnected (Thumb, 4 bytes, Stack size 0 bytes, usbd_core.o(i.USBD_LL_DevConnected))
  [Called By]

  - >> HAL_PCD_ConnectCallback

  USBD_LL_DevDisconnected (Thumb, 22 bytes, Stack size 8 bytes, usbd_core.o(i.USBD_LL_DevDisconnected))
  [Stack]

  - Max Depth = 8
  - Call Chain = USBD_LL_DevDisconnected
  [Called By]
  - >> HAL_PCD_DisconnectCallback

  USBD_LL_GetRxDataSize (Thumb, 8 bytes, Stack size 0 bytes, usbd_conf.o(i.USBD_LL_GetRxDataSize))
  [Calls]

  - >> HAL_PCD_EP_GetRxCount
  [Called By]
  - >> USBD_CDC_DataOut

  USBD_LL_Init (Thumb, 78 bytes, Stack size 8 bytes, usbd_conf.o(i.USBD_LL_Init))
  [Stack]

  - Max Depth = 120
  - Call Chain = USBD_LL_Init ⇒ HAL_PCD_Init ⇒ HAL_PCD_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_PCD_Init
  - >> HAL_PCDEx_SetTxFiFo
  - >> HAL_PCDEx_SetRxFiFo
  [Called By]
  - >> USBD_Init

  USBD_LL_IsStallEP (Thumb, 32 bytes, Stack size 0 bytes, usbd_conf.o(i.USBD_LL_IsStallEP))
  [Called By]

  - >> USBD_StdEPReq

  USBD_LL_IsoINIncomplete (Thumb, 4 bytes, Stack size 0 bytes, usbd_core.o(i.USBD_LL_IsoINIncomplete))
  [Called By]

  - >> HAL_PCD_ISOINIncompleteCallback

  USBD_LL_IsoOUTIncomplete (Thumb, 4 bytes, Stack size 0 bytes, usbd_core.o(i.USBD_LL_IsoOUTIncomplete))
  [Called By]

  - >> HAL_PCD_ISOOUTIncompleteCallback

  USBD_LL_OpenEP (Thumb, 20 bytes, Stack size 8 bytes, usbd_conf.o(i.USBD_LL_OpenEP))
  [Stack]

  - Max Depth = 36
  - Call Chain = USBD_LL_OpenEP ⇒ HAL_PCD_EP_Open ⇒ USB_ActivateEndpoint
  [Calls]
  - >> HAL_PCD_EP_Open
  [Called By]
  - >> USBD_LL_Reset
  - >> USBD_CDC_Init

  USBD_LL_PrepareReceive (Thumb, 14 bytes, Stack size 8 bytes, usbd_conf.o(i.USBD_LL_PrepareReceive))
  [Stack]

  - Max Depth = 44
  - Call Chain = USBD_LL_PrepareReceive ⇒ HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> HAL_PCD_EP_Receive
  [Called By]
  - >> USBD_CDC_ReceivePacket
  - >> USBD_CtlReceiveStatus
  - >> USBD_CtlContinueRx
  - >> USBD_CtlPrepareRx
  - >> USBD_CDC_Init

  USBD_LL_Reset (Thumb, 62 bytes, Stack size 16 bytes, usbd_core.o(i.USBD_LL_Reset))
  [Stack]

  - Max Depth = 52
  - Call Chain = USBD_LL_Reset ⇒ USBD_LL_OpenEP ⇒ HAL_PCD_EP_Open ⇒ USB_ActivateEndpoint
  [Calls]
  - >> USBD_LL_OpenEP
  [Called By]
  - >> HAL_PCD_ResetCallback

  USBD_LL_Resume (Thumb, 12 bytes, Stack size 0 bytes, usbd_core.o(i.USBD_LL_Resume))
  [Called By]

  - >> HAL_PCD_ResumeCallback

  USBD_LL_SOF (Thumb, 24 bytes, Stack size 8 bytes, usbd_core.o(i.USBD_LL_SOF))
  [Stack]

  - Max Depth = 8
  - Call Chain = USBD_LL_SOF
  [Called By]
  - >> HAL_PCD_SOFCallback

  USBD_LL_SetSpeed (Thumb, 6 bytes, Stack size 0 bytes, usbd_core.o(i.USBD_LL_SetSpeed))
  [Called By]

  - >> HAL_PCD_ResetCallback

  USBD_LL_SetUSBAddress (Thumb, 14 bytes, Stack size 8 bytes, usbd_conf.o(i.USBD_LL_SetUSBAddress))
  [Stack]

  - Max Depth = 16
  - Call Chain = USBD_LL_SetUSBAddress ⇒ HAL_PCD_SetAddress
  [Calls]
  - >> HAL_PCD_SetAddress
  [Called By]
  - >> USBD_StdDevReq

  USBD_LL_SetupStage (Thumb, 90 bytes, Stack size 16 bytes, usbd_core.o(i.USBD_LL_SetupStage))
  [Stack]

  - Max Depth = 116
  - Call Chain = USBD_LL_SetupStage ⇒ USBD_StdDevReq ⇒ USBD_GetDescriptor ⇒ USBD_CtlSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_StallEP
  - >> USBD_StdItfReq
  - >> USBD_StdEPReq
  - >> USBD_StdDevReq
  - >> USBD_ParseSetupRequest
  [Called By]
  - >> HAL_PCD_SetupStageCallback

  USBD_LL_StallEP (Thumb, 14 bytes, Stack size 8 bytes, usbd_conf.o(i.USBD_LL_StallEP))
  [Stack]

  - Max Depth = 24
  - Call Chain = USBD_LL_StallEP ⇒ HAL_PCD_EP_SetStall
  [Calls]
  - >> HAL_PCD_EP_SetStall
  [Called By]
  - >> USBD_LL_SetupStage
  - >> USBD_CtlError
  - >> USBD_StdEPReq

  USBD_LL_Start (Thumb, 14 bytes, Stack size 8 bytes, usbd_conf.o(i.USBD_LL_Start))
  [Stack]

  - Max Depth = 40
  - Call Chain = USBD_LL_Start ⇒ HAL_PCD_Start ⇒ USB_DevConnect ⇒ HAL_Delay
  [Calls]
  - >> HAL_PCD_Start
  [Called By]
  - >> USBD_Start

  USBD_LL_Suspend (Thumb, 18 bytes, Stack size 0 bytes, usbd_core.o(i.USBD_LL_Suspend))
  [Called By]

  - >> HAL_PCD_SuspendCallback

  USBD_LL_Transmit (Thumb, 14 bytes, Stack size 8 bytes, usbd_conf.o(i.USBD_LL_Transmit))
  [Stack]

  - Max Depth = 44
  - Call Chain = USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> HAL_PCD_EP_Transmit
  [Called By]
  - >> USBD_CDC_TransmitPacket
  - >> USBD_CtlSendStatus
  - >> USBD_CtlContinueSendData
  - >> USBD_CtlSendData

  USBD_ParseSetupRequest (Thumb, 40 bytes, Stack size 0 bytes, usbd_ctlreq.o(i.USBD_ParseSetupRequest))
  [Called By]

  - >> USBD_LL_SetupStage

  USBD_RegisterClass (Thumb, 16 bytes, Stack size 0 bytes, usbd_core.o(i.USBD_RegisterClass))
  [Called By]

  - >> MX_USB_DEVICE_Init

  USBD_SetClassConfig (Thumb, 22 bytes, Stack size 8 bytes, usbd_core.o(i.USBD_SetClassConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = USBD_SetClassConfig
  [Called By]
  - >> USBD_SetConfig

  USBD_Start (Thumb, 10 bytes, Stack size 8 bytes, usbd_core.o(i.USBD_Start))
  [Stack]

  - Max Depth = 48
  - Call Chain = USBD_Start ⇒ USBD_LL_Start ⇒ HAL_PCD_Start ⇒ USB_DevConnect ⇒ HAL_Delay
  [Calls]
  - >> USBD_LL_Start
  [Called By]
  - >> MX_USB_DEVICE_Init

  USBD_StdDevReq (Thumb, 242 bytes, Stack size 24 bytes, usbd_ctlreq.o(i.USBD_StdDevReq))
  [Stack]

  - Max Depth = 100
  - Call Chain = USBD_StdDevReq ⇒ USBD_GetDescriptor ⇒ USBD_CtlSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_SetUSBAddress
  - >> USBD_CtlError
  - >> USBD_SetConfig
  - >> USBD_GetDescriptor
  - >> USBD_CtlSendStatus
  - >> USBD_CtlSendData
  [Called By]
  - >> USBD_LL_SetupStage

  USBD_StdEPReq (Thumb, 192 bytes, Stack size 16 bytes, usbd_ctlreq.o(i.USBD_StdEPReq))
  [Stack]

  - Max Depth = 68
  - Call Chain = USBD_StdEPReq ⇒ USBD_CtlSendStatus ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_LL_StallEP
  - >> USBD_LL_IsStallEP
  - >> USBD_LL_ClearStallEP
  - >> USBD_CtlError
  - >> USBD_CtlSendStatus
  - >> USBD_CtlSendData
  [Called By]
  - >> USBD_LL_SetupStage

  USBD_StdItfReq (Thumb, 52 bytes, Stack size 16 bytes, usbd_ctlreq.o(i.USBD_StdItfReq))
  [Stack]

  - Max Depth = 68
  - Call Chain = USBD_StdItfReq ⇒ USBD_CtlSendStatus ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_CtlError
  - >> USBD_CtlSendStatus
  [Called By]
  - >> USBD_LL_SetupStage

  USBD_static_free (Thumb, 4 bytes, Stack size 0 bytes, usbd_conf.o(i.USBD_static_free))
  [Stack]

  - Max Depth = 8
  - Call Chain = USBD_static_free ⇒ free
  [Calls]
  - >> free
  [Called By]
  - >> USBD_CDC_DeInit

  USBD_static_malloc (Thumb, 4 bytes, Stack size 0 bytes, usbd_conf.o(i.USBD_static_malloc))
  [Called By]

  - >> USBD_CDC_Init

  USB_ActivateEndpoint (Thumb, 138 bytes, Stack size 12 bytes, stm32f1xx_ll_usb.o(i.USB_ActivateEndpoint))
  [Stack]

  - Max Depth = 12
  - Call Chain = USB_ActivateEndpoint
  [Called By]
  - >> HAL_PCD_EP_Open

  USB_ActivateSetup (Thumb, 52 bytes, Stack size 0 bytes, stm32f1xx_ll_usb.o(i.USB_ActivateSetup))
  [Called By]

  - >> HAL_PCD_IRQHandler

  USB_CoreInit (Thumb, 28 bytes, Stack size 8 bytes, stm32f1xx_ll_usb.o(i.USB_CoreInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = USB_CoreInit
  [Calls]
  - >> USB_CoreReset
  [Called By]
  - >> HAL_PCD_Init

  USB_DeactivateEndpoint (Thumb, 110 bytes, Stack size 12 bytes, stm32f1xx_ll_usb.o(i.USB_DeactivateEndpoint))
  [Stack]

  - Max Depth = 12
  - Call Chain = USB_DeactivateEndpoint
  [Called By]
  - >> HAL_PCD_EP_Close

  USB_DevConnect (Thumb, 24 bytes, Stack size 8 bytes, stm32f1xx_ll_usb.o(i.USB_DevConnect))
  [Stack]

  - Max Depth = 24
  - Call Chain = USB_DevConnect ⇒ HAL_Delay
  [Calls]
  - >> HAL_Delay
  [Called By]
  - >> HAL_PCD_Start

  USB_DevDisconnect (Thumb, 24 bytes, Stack size 8 bytes, stm32f1xx_ll_usb.o(i.USB_DevDisconnect))
  [Stack]

  - Max Depth = 24
  - Call Chain = USB_DevDisconnect ⇒ HAL_Delay
  [Calls]
  - >> HAL_Delay
  [Called By]
  - >> HAL_PCD_Init

  USB_DevInit (Thumb, 270 bytes, Stack size 24 bytes, stm32f1xx_ll_usb.o(i.USB_DevInit))
  [Stack]

  - Max Depth = 24
  - Call Chain = USB_DevInit
  [Calls]
  - >> USB_FlushTxFifo
  - >> USB_FlushRxFifo
  [Called By]
  - >> HAL_PCD_Init

  USB_DisableGlobalInt (Thumb, 12 bytes, Stack size 0 bytes, stm32f1xx_ll_usb.o(i.USB_DisableGlobalInt))
  [Called By]

  - >> HAL_PCD_Init

  USB_EP0StartXfer (Thumb, 280 bytes, Stack size 8 bytes, stm32f1xx_ll_usb.o(i.USB_EP0StartXfer))
  [Stack]

  - Max Depth = 8
  - Call Chain = USB_EP0StartXfer
  [Called By]
  - >> HAL_PCD_EP_Transmit
  - >> HAL_PCD_EP_Receive

  USB_EP0_OutStart (Thumb, 46 bytes, Stack size 0 bytes, stm32f1xx_ll_usb.o(i.USB_EP0_OutStart))
  [Called By]

  - >> HAL_PCD_EP_SetStall
  - >> HAL_PCD_IRQHandler

  USB_EPClearStall (Thumb, 100 bytes, Stack size 0 bytes, stm32f1xx_ll_usb.o(i.USB_EPClearStall))
  [Called By]

  - >> HAL_PCD_EP_ClrStall

  USB_EPSetStall (Thumb, 94 bytes, Stack size 0 bytes, stm32f1xx_ll_usb.o(i.USB_EPSetStall))
  [Called By]

  - >> HAL_PCD_EP_SetStall

  USB_EPStartXfer (Thumb, 496 bytes, Stack size 12 bytes, stm32f1xx_ll_usb.o(i.USB_EPStartXfer))
  [Stack]

  - Max Depth = 20
  - Call Chain = USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USB_WritePacket
  [Called By]
  - >> HAL_PCD_EP_Transmit
  - >> HAL_PCD_EP_Receive

  USB_EnableGlobalInt (Thumb, 12 bytes, Stack size 0 bytes, stm32f1xx_ll_usb.o(i.USB_EnableGlobalInt))
  [Called By]

  - >> HAL_PCD_Start

  USB_FlushRxFifo (Thumb, 28 bytes, Stack size 0 bytes, stm32f1xx_ll_usb.o(i.USB_FlushRxFifo))
  [Called By]

  - >> USB_DevInit

  USB_FlushTxFifo (Thumb, 32 bytes, Stack size 0 bytes, stm32f1xx_ll_usb.o(i.USB_FlushTxFifo))
  [Called By]

  - >> HAL_PCD_IRQHandler
  - >> USB_DevInit

  USB_GetMode (Thumb, 8 bytes, Stack size 0 bytes, stm32f1xx_ll_usb.o(i.USB_GetMode))
  [Called By]

  - >> HAL_PCD_IRQHandler

  USB_ReadDevAllInEpInterrupt (Thumb, 14 bytes, Stack size 0 bytes, stm32f1xx_ll_usb.o(i.USB_ReadDevAllInEpInterrupt))
  [Called By]

  - >> HAL_PCD_IRQHandler

  USB_ReadDevAllOutEpInterrupt (Thumb, 14 bytes, Stack size 0 bytes, stm32f1xx_ll_usb.o(i.USB_ReadDevAllOutEpInterrupt))
  [Called By]

  - >> HAL_PCD_IRQHandler

  USB_ReadDevInEPInterrupt (Thumb, 30 bytes, Stack size 0 bytes, stm32f1xx_ll_usb.o(i.USB_ReadDevInEPInterrupt))
  [Called By]

  - >> HAL_PCD_IRQHandler

  USB_ReadDevOutEPInterrupt (Thumb, 16 bytes, Stack size 0 bytes, stm32f1xx_ll_usb.o(i.USB_ReadDevOutEPInterrupt))
  [Called By]

  - >> HAL_PCD_IRQHandler

  USB_ReadInterrupts (Thumb, 8 bytes, Stack size 0 bytes, stm32f1xx_ll_usb.o(i.USB_ReadInterrupts))
  [Called By]

  - >> HAL_PCD_IRQHandler

  USB_ReadPacket (Thumb, 32 bytes, Stack size 8 bytes, stm32f1xx_ll_usb.o(i.USB_ReadPacket))
  [Stack]

  - Max Depth = 8
  - Call Chain = USB_ReadPacket
  [Called By]
  - >> HAL_PCD_IRQHandler

  USB_SetCurrentMode (Thumb, 44 bytes, Stack size 8 bytes, stm32f1xx_ll_usb.o(i.USB_SetCurrentMode))
  [Stack]

  - Max Depth = 24
  - Call Chain = USB_SetCurrentMode ⇒ HAL_Delay
  [Calls]
  - >> HAL_Delay
  [Called By]
  - >> HAL_PCD_Init

  USB_SetDevAddress (Thumb, 34 bytes, Stack size 0 bytes, stm32f1xx_ll_usb.o(i.USB_SetDevAddress))
  [Called By]

  - >> HAL_PCD_SetAddress

  USB_WritePacket (Thumb, 36 bytes, Stack size 8 bytes, stm32f1xx_ll_usb.o(i.USB_WritePacket))
  [Stack]

  - Max Depth = 8
  - Call Chain = USB_WritePacket
  [Called By]
  - >> USB_EPStartXfer
  - >> PCD_WriteEmptyTxFifo

  Usart2_Send_String (Thumb, 38 bytes, Stack size 8 bytes, main.o(i.Usart2_Send_String))
  [Stack]

  - Max Depth = 8
  - Call Chain = Usart2_Send_String
  [Calls]
  - >> Usart2_Send_symbol
  [Called By]
  - >> main

  Usart2_Send_symbol (Thumb, 16 bytes, Stack size 0 bytes, main.o(i.Usart2_Send_symbol))
  [Called By]

  - >> Usart2_Send_String

  __0sprintf$8 (Thumb, 34 bytes, Stack size 24 bytes, printf8.o(i.__0sprintf$8), UNUSED)
  [Calls]

  - >> _sputc
  - >> _printf_core

  __1sprintf$8 (Thumb, 0 bytes, Stack size 24 bytes, printf8.o(i.__0sprintf$8), UNUSED)

  __2sprintf (Thumb, 0 bytes, Stack size 24 bytes, printf8.o(i.__0sprintf$8))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2sprintf
  [Called By]
  - >> main
  - >> CDC_Receive_FS

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  clear_buffer (Thumb, 22 bytes, Stack size 0 bytes, main.o(i.clear_buffer))
  [Called By]

  - >> main

  free (Thumb, 76 bytes, Stack size 8 bytes, malloc.o(i.free))
  [Stack]

  - Max Depth = 8
  - Call Chain = free
  [Called By]
  - >> USBD_static_free

  halfbyte_to_hexascii (Thumb, 16 bytes, Stack size 0 bytes, main.o(i.halfbyte_to_hexascii))
  [Called By]

  - >> HAL_CAN_RxCpltCallback

  hexascii_to_halfbyte (Thumb, 32 bytes, Stack size 0 bytes, main.o(i.hexascii_to_halfbyte))
  [Called By]

  - >> main
  - >> CDC_Receive_FS

  led_blink (Thumb, 54 bytes, Stack size 16 bytes, main.o(i.led_blink))
  [Stack]

  - Max Depth = 16
  - Call Chain = led_blink
  [Calls]
  - >> Delay_ms
  [Called By]
  - >> main
  - >> HAL_CAN_RxCpltCallback

  main (Thumb, 866 bytes, Stack size 136 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 372
  - Call Chain = main ⇒ SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_UART_Init
  - >> HAL_TIM_Base_Start
  - >> HAL_Init
  - >> HAL_CAN_Receive_IT
  - >> HAL_CAN_ConfigFilter
  - >> usb_access
  - >> string_cmp
  - >> led_blink
  - >> clear_buffer
  - >> Usart2_Send_String
  - >> SystemClock_Config
  - >> Delay_ms
  - >> MX_TIM1_Init
  - >> MX_GPIO_Init
  - >> MX_CAN1_Init
  - >> MX_USB_DEVICE_Init
  - >> hexascii_to_halfbyte
  - >> HAL_CAN_Transmit
  - >> CDC_periodic_callback
  - >> __2sprintf
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  string_cmp (Thumb, 28 bytes, Stack size 8 bytes, main.o(i.string_cmp))
  [Stack]

  - Max Depth = 8
  - Call Chain = string_cmp
  [Called By]
  - >> main

  usb_access (Thumb, 126 bytes, Stack size 16 bytes, main.o(i.usb_access))
  [Stack]

  - Max Depth = 76
  - Call Chain = usb_access ⇒ CDC_Transmit_FS ⇒ USBD_CDC_TransmitPacket ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> CDC_Transmit_FS
  [Called By]
  - >> main

  ### Local Symbols

  CDC_Control_FS (Thumb, 4 bytes, Stack size 0 bytes, usbd_cdc_if.o(i.CDC_Control_FS))
  [Address Reference Count : 1]

  - usbd_cdc_if.o(.data)

  CDC_DeInit_FS (Thumb, 4 bytes, Stack size 0 bytes, usbd_cdc_if.o(i.CDC_DeInit_FS))
  [Address Reference Count : 1]

  - usbd_cdc_if.o(.data)

  CDC_Init_FS (Thumb, 28 bytes, Stack size 8 bytes, usbd_cdc_if.o(i.CDC_Init_FS))
  [Stack]

  - Max Depth = 8
  - Call Chain = CDC_Init_FS
  [Calls]
  - >> USBD_CDC_SetTxBuffer
  - >> USBD_CDC_SetRxBuffer
  [Address Reference Count : 1]
  - usbd_cdc_if.o(.data)

  CDC_Receive_FS (Thumb, 354 bytes, Stack size 24 bytes, usbd_cdc_if.o(i.CDC_Receive_FS))
  [Stack]

  - Max Depth = 76
  - Call Chain = CDC_Receive_FS ⇒ USBD_CDC_ReceivePacket ⇒ USBD_LL_PrepareReceive ⇒ HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> hexascii_to_halfbyte
  - >> USBD_CDC_SetRxBuffer
  - >> USBD_CDC_ReceivePacket
  - >> HAL_CAN_Transmit
  - >> __2sprintf
  [Address Reference Count : 1]
  - usbd_cdc_if.o(.data)

  MX_CAN1_Init (Thumb, 48 bytes, Stack size 0 bytes, main.o(i.MX_CAN1_Init))
  [Stack]

  - Max Depth = 96
  - Call Chain = MX_CAN1_Init ⇒ HAL_CAN_Init ⇒ HAL_CAN_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_CAN_Init
  [Called By]
  - >> main

  MX_GPIO_Init (Thumb, 128 bytes, Stack size 40 bytes, main.o(i.MX_GPIO_Init))
  [Stack]

  - Max Depth = 80
  - Call Chain = MX_GPIO_Init ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> main

  MX_TIM1_Init (Thumb, 64 bytes, Stack size 32 bytes, main.o(i.MX_TIM1_Init))
  [Stack]

  - Max Depth = 60
  - Call Chain = MX_TIM1_Init ⇒ HAL_TIM_Base_Init ⇒ TIM_Base_SetConfig
  [Calls]
  - >> HAL_TIM_ConfigClockSource
  - >> HAL_TIM_Base_Init
  - >> HAL_TIMEx_MasterConfigSynchronization
  [Called By]
  - >> main

  USBD_CDC_DataIn (Thumb, 20 bytes, Stack size 0 bytes, usbd_cdc.o(i.USBD_CDC_DataIn))
  [Address Reference Count : 1]

  - usbd_cdc.o(.data)

  USBD_CDC_DataOut (Thumb, 46 bytes, Stack size 16 bytes, usbd_cdc.o(i.USBD_CDC_DataOut))
  [Stack]

  - Max Depth = 16
  - Call Chain = USBD_CDC_DataOut
  [Calls]
  - >> USBD_LL_GetRxDataSize
  [Address Reference Count : 1]
  - usbd_cdc.o(.data)

  USBD_CDC_DeInit (Thumb, 60 bytes, Stack size 16 bytes, usbd_cdc.o(i.USBD_CDC_DeInit))
  [Stack]

  - Max Depth = 44
  - Call Chain = USBD_CDC_DeInit ⇒ USBD_LL_CloseEP ⇒ HAL_PCD_EP_Close ⇒ USB_DeactivateEndpoint
  [Calls]
  - >> USBD_static_free
  - >> USBD_LL_CloseEP
  [Address Reference Count : 1]
  - usbd_cdc.o(.data)

  USBD_CDC_EP0_RxReady (Thumb, 36 bytes, Stack size 8 bytes, usbd_cdc.o(i.USBD_CDC_EP0_RxReady))
  [Stack]

  - Max Depth = 8
  - Call Chain = USBD_CDC_EP0_RxReady
  [Address Reference Count : 1]
  - usbd_cdc.o(.data)

  USBD_CDC_GetFSCfgDesc (Thumb, 8 bytes, Stack size 0 bytes, usbd_cdc.o(i.USBD_CDC_GetFSCfgDesc))
  [Address Reference Count : 1]

  - usbd_cdc.o(.data)

  USBD_CDC_GetHSCfgDesc (Thumb, 8 bytes, Stack size 0 bytes, usbd_cdc.o(i.USBD_CDC_GetHSCfgDesc))
  [Address Reference Count : 1]

  - usbd_cdc.o(.data)

  USBD_CDC_GetOtherSpeedCfgDesc (Thumb, 8 bytes, Stack size 0 bytes, usbd_cdc.o(i.USBD_CDC_GetOtherSpeedCfgDesc))
  [Address Reference Count : 1]

  - usbd_cdc.o(.data)

  USBD_CDC_Init (Thumb, 136 bytes, Stack size 24 bytes, usbd_cdc.o(i.USBD_CDC_Init))
  [Stack]

  - Max Depth = 68
  - Call Chain = USBD_CDC_Init ⇒ USBD_LL_PrepareReceive ⇒ HAL_PCD_EP_Receive ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_static_malloc
  - >> USBD_LL_PrepareReceive
  - >> USBD_LL_OpenEP
  [Address Reference Count : 1]
  - usbd_cdc.o(.data)

  USBD_CDC_Setup (Thumb, 92 bytes, Stack size 16 bytes, usbd_cdc.o(i.USBD_CDC_Setup))
  [Stack]

  - Max Depth = 68
  - Call Chain = USBD_CDC_Setup ⇒ USBD_CtlSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_CtlSendData
  - >> USBD_CtlPrepareRx
  [Address Reference Count : 1]
  - usbd_cdc.o(.data)

  USBD_GetDescriptor (Thumb, 224 bytes, Stack size 24 bytes, usbd_ctlreq.o(i.USBD_GetDescriptor))
  [Stack]

  - Max Depth = 76
  - Call Chain = USBD_GetDescriptor ⇒ USBD_CtlSendData ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_CtlError
  - >> USBD_CtlSendData
  [Called By]
  - >> USBD_StdDevReq

  USBD_SetConfig (Thumb, 110 bytes, Stack size 16 bytes, usbd_ctlreq.o(i.USBD_SetConfig))
  [Stack]

  - Max Depth = 68
  - Call Chain = USBD_SetConfig ⇒ USBD_CtlSendStatus ⇒ USBD_LL_Transmit ⇒ HAL_PCD_EP_Transmit ⇒ USB_EPStartXfer ⇒ USB_WritePacket
  [Calls]
  - >> USBD_CtlError
  - >> USBD_CtlSendStatus
  - >> USBD_SetClassConfig
  - >> USBD_ClrClassConfig
  [Called By]
  - >> USBD_StdDevReq

  NVIC_SetPriority (Thumb, 32 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.NVIC_SetPriority))
  [Called By]

  - >> HAL_NVIC_SetPriority
  - >> HAL_SYSTICK_Config

  USB_CoreReset (Thumb, 70 bytes, Stack size 0 bytes, stm32f1xx_ll_usb.o(i.USB_CoreReset))
  [Called By]

  - >> USB_CoreInit

  PCD_WriteEmptyTxFifo (Thumb, 142 bytes, Stack size 32 bytes, stm32f1xx_hal_pcd.o(i.PCD_WriteEmptyTxFifo))
  [Stack]

  - Max Depth = 40
  - Call Chain = PCD_WriteEmptyTxFifo ⇒ USB_WritePacket
  [Calls]
  - >> USB_WritePacket
  [Called By]
  - >> HAL_PCD_IRQHandler

  CAN_Receive_IT (Thumb, 276 bytes, Stack size 8 bytes, stm32f1xx_hal_can.o(i.CAN_Receive_IT))
  [Stack]

  - Max Depth = 232
  - Call Chain = CAN_Receive_IT ⇒ HAL_CAN_RxCpltCallback ⇒ led_blink
  [Calls]
  - >> HAL_CAN_RxCpltCallback
  [Called By]
  - >> HAL_CAN_IRQHandler

  TIM_ETR_SetConfig (Thumb, 20 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.TIM_ETR_SetConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_ETR_SetConfig
  [Called By]
  - >> HAL_TIM_ConfigClockSource

  TIM_ITRx_SetConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.TIM_ITRx_SetConfig))
  [Called By]

  - >> HAL_TIM_ConfigClockSource

  TIM_TI1_ConfigInputStage (Thumb, 34 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.TIM_TI1_ConfigInputStage))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_TI1_ConfigInputStage
  [Called By]
  - >> HAL_TIM_ConfigClockSource

  TIM_TI2_ConfigInputStage (Thumb, 36 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.TIM_TI2_ConfigInputStage))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_TI2_ConfigInputStage
  [Called By]
  - >> HAL_TIM_ConfigClockSource

  UART_SetConfig (Thumb, 220 bytes, Stack size 24 bytes, stm32f1xx_hal_uart.o(i.UART_SetConfig))
  [Stack]

  - Max Depth = 100
  - Call Chain = UART_SetConfig ⇒ HAL_RCC_GetPCLK2Freq ⇒ HAL_RCC_GetHCLKFreq ⇒ HAL_RCC_GetSysClockFreq
  [Calls]
  - >> HAL_RCC_GetPCLK2Freq
  - >> HAL_RCC_GetPCLK1Freq
  [Called By]
  - >> HAL_UART_Init

  _printf_core (Thumb, 996 bytes, Stack size 104 bytes, printf8.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uldivmod
  - >> _printf_pre_padding
  - >> _printf_post_padding
  [Called By]
  - >> __0sprintf$8

  _printf_post_padding (Thumb, 36 bytes, Stack size 24 bytes, printf8.o(i._printf_post_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _printf_pre_padding (Thumb, 46 bytes, Stack size 24 bytes, printf8.o(i._printf_pre_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _sputc (Thumb, 10 bytes, Stack size 0 bytes, printf8.o(i._sputc))
  [Called By]

  - >> __0sprintf$8
  [Address Reference Count : 1]
  - printf8.o(i.__0sprintf$8)

  ### Undefined Global Symbols