Adaption Additive Bank 1,ADD,ms,12050B06
Adaption Additive Bank 1,LAMBDA_ADD_1,ms,12050B06
Adaption Additive Bank 2,ADD_2,ms,12050B06
Adaption Additive Bank 2,LAMBDA_ADD_2,ms,12050B06
Exhaust camshaft pos. bank 1 actual,AVANOS1_IST,Deg. KW,12050B23
Exhaust camshaft pos. bank 2 actual,AVANOS2_IST,Deg. KW,12050B23
Exhaust camshaft pos. bank 1 expected,AVANOS1_SOLL,Deg. KW,12050B23
Exhaust camshaft pos. bank 2 actual,AVANOS2_SOLL,Deg. KW,12050B23
relativer Oeffnungsquerschnitt,AQREL,%,12050B03
Throttle pos. actual,DKP_WINKEL,%,12050B03
Throttle pos. expected,DKP_WINKEL_SOLL,%,12050B03
Intake camshaft pos. bank 1 actual,EVANOS1_IST,Deg. KW,12050B23
Intake camshaft pos. bank 2 actual,EVANOS2_IST,Deg. KW,12050B23
Intake camshaft pos. bank 1 expected,EVANOS1_SOLL,Deg. KW,12050B23
Intake camshaft pos. bank 2 expected,EVANOS2_SOLL,Deg. KW,12050B23
TPS 1,PWG_POTI_WINKEL,%,12050B03
TPS 2,PWG_POTI_WINKEL_2,%,12050B03
Lambdaintegrator 1,LAMBDA_INTEGRATOR_1,[1],12050B13
Lambdaintegrator 1,INT,[1],12050B13
Lambdaintegrator 2,LAMBDA_INTEGRATOR_2,[1],12050B13
Lambdaintegrator 2,INT2,[1],12050B13
Idle controller adaptation with compressor,LFR_KO,Nm,12050B06
Idle controller adaptation without compressor,LFR,Nm,12050B06
Lambda 1 post cat voltage ,LS_NKAT_SIGNAL_1,V,12050B02
Lambda 1 post cat voltage ,L_SONDE_H,V,12050B02
Lambda 2 post cat voltage ,LS_NKAT_SIGNAL_2,V,12050B02
Lambda 2 post cat voltage ,L_SONDE_2_H,V,12050B02
Lambda 1 pre cat voltage ,LS_VKAT_SIGNAL_1,V,12050B02
Lambda 1 pre cat voltage ,L_SONDE,V,12050B02
Lambda 2 pre cat voltage ,LS_VKAT_SIGNAL_2,V,12050B02
Lambda 2 pre cat voltage ,L_SONDE_2,V,12050B02
TPS 1 Voltage,PWG_POTI_SPANNUNG,V,12050B02
MAF ,LMM_MASSE,kg/h,12050B03
Adaptation Multiplicative Bank 1,LAMBDA_MUL_1,[1],12050B06
Adaptation Multiplicative Bank 1,MUL,[1],12050B06
Adaptation Multiplicative Bank 2,LAMBDA_MUL_2,[1],12050B06
Adaptation Multiplicative Bank 2,MUL_2,[1],12050B06
RPM,MOTORDREHZAHL,1/min,12050B03
Max RPM,NMAX,km/h,12050B06
Idle controller expected RPM,N_LL_SOLL,1/min,12050B03
Environment pressure (intern),PUMG_INTERN,mbar,12050B03
relative Fuellung,RF,%,12050B03
Exhaust temp.,TABG,Deg C,12050B03
Intake temp.,AN_LUFTTEMPERATUR,Deg C,12050B03
Injection time cyl. 1,EINSPRITZZEIT,ms,12050B13
Injection time cyl. 2,TI2,ms,12050B13
Injection time cyl. 3,TI3,ms,12050B13
Injection time cyl. 4,TI4,ms,12050B13
Injection time cyl. 5,TI5,ms,12050B13
Injection time cyl. 6,TI6,ms,12050B13
Injection time cyl. 7,TI7,ms,12050B13
Injection time cyl. 8,TI8,ms,12050B13
Ausblendzaehler Einspritzung Ist,TI_AUS_IST,[1],12050B13
Ist Strom Servotronikventil,STATUS_ANALOG_GM3,mA,12050B13
Soll Strom Servotronikventil,STATUS_ANALOG_GM3,mA,12050B13
Soll Strom Servotronikventil,STATUS_ANALOG_GM3,%,12050B15
Coolant temp.,KUEHLW_AUSL_TEMPERATUR,GradC,12050B03
load signal,LAST,ms,12050B03
Motor temp.,MOTORTEMPERATUR,Deg C,12050B03
Gesamtzeit Ueberdrehzahl n,TNMAX,s,12050B06
Oil temp. (TOG),OEL_TEMPERATUR,Deg C,12050B03
Environment temp.,TUMG,Deg C,12050B03
Tank ventilation valve duty cycle,TV_TEV,ms,12050B13
Ignition angle cyl. 1,TZ1,Deg. KW,12050B13
Ignition angle cyl. 2,TZ2,Deg. KW,12050B13
Ignition angle cyl. 3,TZ3,Deg. KW,12050B13
Ignition angle cyl. 4,TZ4,Deg. KW,12050B13
Ignition angle cyl. 5,TZ5,Deg. KW,12050B13
Ignition angle cyl. 6,TZ6,Deg. KW,12050B13
Ignition angle cyl. 7,TZ7,Deg. KW,12050B13
Ignition angle cyl. 8,TZ8,Deg. KW,12050B13
Battery voltage,UBATT,V,12050B03
Sensorversorgung 1 (Master),UEXT1,V,12050B03
Sensorversorgung 2 (Slave),UEXT2,V,12050B03
Vehicle speed,GESCHWINDIGKEIT,km/h,12050B13
Fahrzeuggeschwindigkeit v_asc (CAN),V_CAN,km/h,12050B13
TEV Messstrom,TEV Messstrom,,12050B13
TEV Messzeit,TEV Messzeit,s,12050B13
Max. speed,VMAX,km/h,12050B06
