<CSVFile>
  <columns>
	<column>
		<number>1</number>
		<ecu>D60M57A0</ecu>
		<jobname>MW_SELECT_LESEN_NORM</jobname>
		<virtualjob>SET_1</virtualjob>
		<resultname>STAT_AFSCD_DMAIRNORM_WERT</resultname>
	</column>
	<column>
		<number>2</number>
		<ecu>D60M57A0</ecu>
		<jobname>MW_SELECT_LESEN_NORM</jobname>
		<virtualjob>SET_1</virtualjob>
		<resultname>STAT_AFSCD_MAIRPERCYL_WERT</resultname>
	</column>
	<column>
		<number>3</number>
		<ecu>D60M57A0</ecu>
		<jobname>MW_SELECT_LESEN_NORM</jobname>
		<virtualjob>SET_1</virtualjob>
		<resultname>STAT_AIRCTL_MDESVAL_WERT</resultname>
	</column>
	<column>
		<number>4</number>
		<ecu>D60M57A0</ecu>
		<jobname>MW_SELECT_LESEN_NORM</jobname>
		<virtualjob>SET_1</virtualjob>
		<resultname>STAT_APPCD_RFLT_WERT</resultname>
	</column>
	<column>
		<number>5</number>
		<ecu>D60M57A0</ecu>
		<jobname>MW_SELECT_LESEN_NORM</jobname>
		<virtualjob>SET_1</virtualjob>
		<resultname>STAT_BATTCD_U_WERT</resultname>
	</column>
	<column>
		<number>6</number>
		<ecu>D60M57A0</ecu>
		<jobname>MW_SELECT_LESEN_NORM</jobname>
		<virtualjob>SET_1</virtualjob>
		<resultname>STAT_BPSCD_POUTVAL_WERT</resultname>
	</column>
	<column>
		<number>7</number>
		<ecu>D60M57A0</ecu>
		<jobname>MW_SELECT_LESEN_NORM</jobname>
		<virtualjob>SET_1</virtualjob>
		<resultname>STAT_COENG_TRQ_WERT</resultname>
	</column>
	<column>
		<number>8</number>
		<ecu>D60M57A0</ecu>
		<jobname>MW_SELECT_LESEN_NORM</jobname>
		<virtualjob>SET_1</virtualjob>
		<resultname>STAT_CRCTL_NUMGEAR_WERT</resultname>
	</column>
	<column>
		<number>9</number>
		<ecu>D60M57A0</ecu>
		<jobname>MW_SELECT_LESEN_NORM</jobname>
		<virtualjob>SET_1</virtualjob>
		<resultname>STAT_CTSCD_TCLNT_WERT</resultname>
	</column>
	<column>
		<number>10</number>
		<ecu>D60M57A0</ecu>
		<jobname>MW_SELECT_LESEN_NORM</jobname>
		<virtualjob>SET_1</virtualjob>
		<resultname>STAT_EGRCD_ROUT_WERT</resultname>
	</column>
	<column>
		<number>11</number>
		<ecu>D60M57A0</ecu>
		<jobname>MW_SELECT_LESEN_NORM</jobname>
		<virtualjob>SET_1</virtualjob>
		<resultname>STAT_ENG_NAVRG_CARB_WERT</resultname>
	</column>
	<column>
		<number>12</number>
		<ecu>D60M57A0</ecu>
		<jobname>MW_SELECT_LESEN_NORM</jobname>
		<virtualjob>SET_1</virtualjob>
		<resultname>STAT_FTSCD_TFUEL_WERT</resultname>
	</column>
	<column>
		<number>13</number>
		<ecu>D60M57A0</ecu>
		<jobname>MW_SELECT_LESEN_NORM</jobname>
		<virtualjob>SET_1</virtualjob>
		<resultname>STAT_GEARBX_STGEAR_WERT</resultname>
	</column>	
	<column>
		<number>14</number>
		<ecu>D60M57A0</ecu>
		<jobname>MW_SELECT_LESEN_NORM</jobname>
		<virtualjob>SET_1</virtualjob>
		<resultname>STAT_IATSCD_TAIRCATS_WERT</resultname>
	</column>
	<column>
		<number>15</number>
		<ecu>D60M57A0</ecu>
		<jobname>MW_SELECT_LESEN_NORM</jobname>
		<virtualjob>SET_1</virtualjob>
		<resultname>STAT_LSU_RLMBD[0]_WERT</resultname>
	</column>
	<column>
		<number>16</number>
		<ecu>D60M57A0</ecu>
		<jobname>MW_SELECT_LESEN_NORM</jobname>
		<virtualjob>SET_1</virtualjob>
		<resultname>STAT_OXICCD_TPRE_WERT</resultname>
	</column>
	<column>
		<number>17</number>
		<ecu>D60M57A0</ecu>
		<jobname>MW_SELECT_LESEN_NORM</jobname>
		<virtualjob>SET_1</virtualjob>
		<resultname>STAT_PCR_PBDESLP_MP_WERT</resultname>
	</column>
	<column>
		<number>18</number>
		<ecu>D60M57A0</ecu>
		<jobname>MW_SELECT_LESEN_NORM</jobname>
		<virtualjob>SET_1</virtualjob>
		<resultname>STAT_PFLTCD_PPRE_WERT</resultname>
	</column>
	<column>
		<number>19</number>
		<ecu>D60M57A0</ecu>
		<jobname>MW_SELECT_LESEN_NORM</jobname>
		<virtualjob>SET_1</virtualjob>
		<resultname>STAT_RAILCD_PPEAK_WERT</resultname>
	</column>
	<column>
		<number>20</number>
		<ecu>D60M57A0</ecu>
		<jobname>MW_SELECT_LESEN_NORM</jobname>
		<virtualjob>SET_1</virtualjob>
		<resultname>STAT_RAIL_PSETPOINT_WERT</resultname>
	</column>

  </columns>
</CSVFile>